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Audi A4 Current Flow Diagram No. 49/1

Edition 05.2003

Continuously variable automatic gearbox: multitronic 01J ®
From model year 2002

Main fuse

¢ On battery

Fuse box

+ Dash panel, driver's side
Fuse colours

30 A -green

25 A - white

20 A - yellow

15 A - blue

10 A -red
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+ In electronics box, plenum chamber
1 - 10-pin connector, black (T10)
2 - 10-pin connector, brown (T10a)
3 - 17-pin connector, red (T17d)
6 - 17-pin connector, white (T17e)

4-point relay carrier

+ In electronics box, plenum chamber
1 - Automatic gearbox relay
4 - Starter inhibitor and reversing light relay
C - Automatic gearbox fuse (for ATF pump run-on)

4-point relay carrier with screw connection
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ws = white
sw = black
ro =red

br = brown
gn = green
bl = blue
gr =grey

i = purple
ge = yellow
or = orange
rs = pink
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No. 49/2

Voltage supply, starter inhibitor and reversing light relay
B - Starter

D Ignition/starter switch

J217 Automatic gearbox control unit m

J226 - Starter inhibitor and reversing light relay

M16 - Reversing light bulb, left
M17 - Reversing light bulb, right
S5 -

Fuse in fuse box/relay plate

$231 - Fuse in fuse box &1

T Single connector, black, engine compartment, right

T10a - 10-pin connector, brown, connector point, electronics box,
plenum chamber

T17d - 17-pin connector, red, connector point, electronics box,
plenum chamber
501 - Screw connection -2- (30), on relay plate
A2 - Positive (+) connection (15), in dash panel wiring harness
A2 " Positive (+) connection (30), in dash panel wiring harness
A0 " Connection (15a, fuse 231), in dash panel wiring harness
A7 " Connection (RF (reversing light)), in dash panel wiring
harness
b5t Positive (+) connection -1- (15), in engine compartment

wiring harness

- Only applies to models with 2.4 litre Motronic
- For 1.8 litre and 2.0 litre engine: connector T1d
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Audi A4 Current Flow Diagram No. 49/3

Automatic gearbox control unit, Tiptronic switch
E1 - Lighting switch

F189 - Tiptronic switch
{ } J6o - Automatic gearbox relay
J217 - Automatic gearbox control unit m
@ » N110 - Selector lever lock solenoid
$286 - Automatic gearbox fuse (for ATF pump run-on) ﬁ
T10j - 10-pin connector, black, on Tiptronic switch

T17e - 17-pin connector, white, connector point, electronics box,
plenum chamber
Earth connection -1-, in front right wiring harness

pPPP ¢ >

83
o5 236 - Earth connection -1-, in interior wiring harness
wibl
a7 “fo
{ ® / } 500 - Screw connection -1- (30), on relay plate
l7 T
05 R T Er A3 - Positive (+) connection (58), in dash panel wiring harness
Sar G g oor |
oas A4 Connection (15a, fuse 5), in dash panel wiring harness
Tizen TI7eBT17e [ T17e () - " . . -
] l myny - pso - Positive (+) connection (30), in engine compartment wiring
ws = white hamess
Sor St =R R o oige Dia.ﬁ sw = black # - Only applies to models with 2.4 litre Motronic
o Mosleoehios  bnorhioe  Jrgro to =ted
br = brown
| an = green
J Fas bl = blue
ar =grey
i = purple
ge = yellow
or =orange
rs = pink
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No. 49/4

Automatic gearbox control unit, automatic gearbox fuse (for ATF
pump run-on)

Jo.

J217
» 5286

12
83

D173

ws = white
sw = black
ro =red

br = brown
gn = green
bl = blue
gr =grey

i = purple
ge = yellow
or = orange
rs = pink

Engine management system relay (see applicable engine
Current Flow Diagram)

Automatic gearbox control unit (o]

Automatic gearbox fuse (for ATF pump run-on) m

Earth point, in engine compartment, left

Earth connection -1-, in front right wiring harness
Connection (87), in engine prewiring wiring harness

Only applies to models with petrol engine (1.8 litre)
Only applies to models with petrol engine (2.0 litre)
Only applies to models with petrol engine (3.0 litre)
Only applies to models with diesel engine (1.9 litre - TDI)
Only applies to models with diesel engine (2.5 litre - TDI)
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No. 49/5

Automatic gearbox control unit, dash panel insert

Jo.
J217
J285
T10
T10a

T16
T17d

T32a
A19

A76

A121
A122
D159

D160

Engine control units
Automatic gearbox control unit

Control unit with display in dash panel insert (0]

10-pin connector, black, connector point, electronics box,
plenum chamber

10-pin connector, brown, connector point, electronics box,
plenum chamber

16-pin connector, black, diagnostic connector

17-pin connector, red, connector point, electronics box,
plenum chamber

32-pin connector, green, on dash panel insert
Connection (58d), in dash panel wiring harness

Connection (diagnosis wire K), in dash panel wiring harness
Connection (high bus), in dash panel wiring harness
Connection (low bus), in dash panel wiring harness
Connection (high bus), in engine compartment wiring harness
Connection (low bus), in engine compartment wiring harness
Only applies to models with diesel engine or 2.0 litre FSI

engine, = applicable engine Current Flow Diagram
Only applies to models with petrol engine





