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Notes:

= — The heater rating plate indicates the version concemed
~ Type "2/C-D" with circulation pump -V55 = auxiliary heater or auxiliary heater with additional heater (for vehicles with diesel engine only)
- Type "2/C-8" vith circulation pump -V55 = auxiliary heater (for vehicles with petrol engine only)

= Auxiliry heater control functions remain in operation during seffdiagnosis

= — Adapter VAS 6017 is required for performing seff-diagnosis on vehicles as of Model Year 2002. On these vehicles, diagnostic wire to auxiliary heater
is connected to a diflerent diagnostic connector contact.

On vehicles with diesel engine, the additional heater or auxiliary heater additional heating function is switched on by the engine control unit each time the
vehicle is started s soon as the following conditions are met.

- Engine speed greater than 600 rpm

- Ambient temperature less than +5 °C

- Air conditioner not set to "Econ” mode

- Coolant temperature less than 70° C to 80° C (depending on ambient temperature)

=> Relevant diesel direct-injection and glow plug system workshop manual: Repair group 01 Reading measured value block

- Heater control unit -J162 adapted in adaption channel "10" with "0" or "2" as additional heater =>Page 01-125 (applies to auxiliary heaters with control
unit as of software version "D§0")

On vehicles with 8-cyl engine and small coolant circuit (gradual introduction as of Model Year 2002), auxiliary heater circulation pump -V55 is switched on
each time cold engine is started if earth is applied to auxiliary heater by coolant shut-off valve relay J541. Prerequisite:

- Heater control unit -J162 adapted in adaption channel "10" with "1" or "3" =>Page 01-125 (applies to auxiliary heaters with control unit as of software
version "D50")
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HEIZGERAT Typ Thermo Top Z/C-
Spannung /El. Leistung 12V /45W
‘Warmestrom SkW_
Brennstoff Benzin
2ul. Betriebsiiberdruck 2.5 bar
Prufzeichen MW S
Fabriknummer
Inbetriebnahmejahr 19 96 97 98
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